

ES160 PROVERS

Features

• Attractive classical oven design creating authentic ambience in sales areas

• Setting up either independently or in combination with Eloma bake ovens BACKMASTER ® to form efficient baking stations

• Large panorama view glass door - design matches Eloma BACKMASTER ®

• Compact dimensions - horizontal controls for limited spaces

• Easy and safe operation

• Clear foil control panel with large digital displays

• Optimal moisture regulation, digital setting from 40% to 90%

• Digital temperature setting from 20° C to 50° C

• Timer 0-99 minutes

• Acoustic sound signal

• Brightly illuminated oven cavity - 4 halogen lamps

• Magnetic door lock - one hand operation - smooth locking and opening

• Automatic water feed with audible and visible indication of water shortage

Construction

• All interior and exterior parts chrome nickel steel CrNi 18 10 - material No. 1.4301

• Security glass panorama door

• Temperature range 20° C to 50°C

• Container collecting condensed water fixed on the outside of the appliance

• Vertically adjustable feet

• Built and controlled in Germany according to quality management system EN ISO 9001

Optional extras


• Doors left-hand hinged, no extra charge

• Caster wheels